
1. **Update BMC firmware to L1.48**


**Step 1.**

**Enter the IP address in the browser, the user name and password default to "admin"**

****


**Step 2.**

**Select “maintenance” and “Firmware Update”**

****

**Step 3.**


**Upload “ROMED8QM-2T\_L1.48.00.ima” and click “Start firmware update”**

****

**Update CPLD to R0.09**


**Step 1.**

**Select “maintenance” and “BPB CPLD Update”**

****

**Step 2.**

**Upload “1U10E\_BPB\_R009.jed” and click “Start firmware update”**

****