

**PLX SOP**


**How to check the speed of PCIE Upstream and Downstream**


Prepare:

1. JavaSetup8u40.exe
2. PLX\_SDK\_v7\_11\_Final\_2014-03-04.exe
3. AsRock\_8747-8748-8732.lic


Steps:

1. Install JAVA
2. Install “PLX\_SDK\_v7\_11\_Final\_2014-03-04.exe”
3. Execute “PLX Device Editor”
4. Select License file and load it.





1. Execute CUDA\_DMA to stress PCIE card.



1. Execute “PLX Device Editor”.

Check value of port 0(upstream) and port 16(downstream), normal link speed is GEN-3 and #Active is 16

