# Results for c:\Test Report\Report\G4PCIE_EX10_R2.00\Report\PCIE Gen 4\PCIE 10\PCIE10_LANE 7_P0

Sigtest:

- Overall Sigtest Result: Pass!

- Mean Unit Interval (ps): 62.502279

- Min Time Between Crossovers (ps): 31.733046

- Data Rate (Gb/s): 15.999417

- Max Peak to Peak Jitter: 29.098618 ps

- Total Jitter at BER of 10E-12: 35.99053 ps
  Total Jitter at BER of 10E-12 Passes Sigtest Limits!

- Minimum eye width: 26.50947 ps

- Deterministic Jitter Delta-Delta: 7.767451 ps
  Deterministic Jitter Delta-Delta Passes Sigtest Limits!

- Random Jitter (RMS): 2.00605 ps
  Random Jitter (RMS) Passes Sigtest Limits!

- Minimum Transition Eye Voltage: -0.137314 volts
  Minimum Transition Eye Voltage Passes Sigtest Limits!

- Maximum Transition Eye Voltage: 0.132532 volts
  Maximum Transition Eye Voltage Passes Sigtest Limits!

- Composite Eye Height: 0.066693

- Composite Eye Location: 0.484
  Composite Eye Height Passes Sigtest Limits!

- Extrapolated Eye Height: 0.057138
  Extrapolated Eye Height Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Above Eye: 0.031436 volts
  Minimum Transition Eye Voltage Margin Above Eye Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Below Eye: -0.040093 volts
  Minimum Transition Eye Voltage Margin Below Eye Passes Sigtest Limits!

- Minimum Transition Eye Height: 0.090529 volts

Worst Non Transition Signal Eye

TEMPLATE FILE SETTINGS

- Template File: PCIE_4_0_SYS \ PCIE_4_16GB_CEM_DUAL_PORT

- Nominal Data Rate (bits/sec): 15999999999.999998

- Target Unit Interval (s): 6.25e-011

- Minimum Time Allowed Between Crossovers (s): 4.0e-011

- Minimum Data For Testing (UI): 200

- Ambiguous UI Resolution Method: EYE_AMBIGUOUS_NONE (0)

- Tj@E-12 Peak to Peak Jitter Limit (s): 4.075e-011

- CTLE equalization index = 1

- DFE equalization: Tap 1 = 20.019531, Tap 2 = -7.8125

  Sigtest Version: 4.0.51