# Results for c:\Users\Administrator\Desktop\project\Jack\G4PCIE_EX10_V1.00\PCIE GEN 4\PCIE 4\PCIE4 LANE7_P0

Sigtest:

- Overall Sigtest Result: Pass!

- Mean Unit Interval (ps): 62.50269

- Min Time Between Crossovers (ps): 28.48025

- Data Rate (Gb/s): 15.999311

- Max Peak to Peak Jitter: 28.481567 ps

- Total Jitter at BER of 10E-12: 33.354808 ps
  Total Jitter at BER of 10E-12 Passes Sigtest Limits!

- Minimum eye width: 29.145192 ps

- Deterministic Jitter Delta-Delta: 7.684434 ps
  Deterministic Jitter Delta-Delta Passes Sigtest Limits!

- Random Jitter (RMS): 1.824608 ps
  Random Jitter (RMS) Passes Sigtest Limits!

- Minimum Transition Eye Voltage: -0.125336 volts
  Minimum Transition Eye Voltage Passes Sigtest Limits!

- Maximum Transition Eye Voltage: 0.119086 volts
  Maximum Transition Eye Voltage Passes Sigtest Limits!

- Composite Eye Height: 0.060724

- Composite Eye Location: 0.476
  Composite Eye Height Passes Sigtest Limits!

- Extrapolated Eye Height: 0.040264
  Extrapolated Eye Height Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Above Eye: 0.028684 volts
  Minimum Transition Eye Voltage Margin Above Eye Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Below Eye: -0.03396 volts
  Minimum Transition Eye Voltage Margin Below Eye Passes Sigtest Limits!

- Minimum Transition Eye Height: 0.081644 volts

Worst Non Transition Signal Eye

TEMPLATE FILE SETTINGS

- Template File: PCIE_4_0_SYS \ PCIE_4_16GB_CEM_DUAL_PORT

- Nominal Data Rate (bits/sec): 15999999999.999998

- Target Unit Interval (s): 6.25e-011

- Minimum Time Allowed Between Crossovers (s): 4.0e-011

- Minimum Data For Testing (UI): 200

- Ambiguous UI Resolution Method: EYE_AMBIGUOUS_NONE (0)

- Tj@E-12 Peak to Peak Jitter Limit (s): 4.075e-011

- CTLE equalization index = 1

- DFE equalization: Tap 1 = 21.484375, Tap 2 = -5.859375

  Sigtest Version: 4.0.51