# Results for c:\Users\Administrator\Desktop\Project\G4PCIE_EX10_V2.00\PCIE Gen 4\PCIE 3\PCIE3_LANE 15_P0

Sigtest:

- Overall Sigtest Result: Pass!

- Mean Unit Interval (ps): 62.502737

- Min Time Between Crossovers (ps): 33.344135

- Data Rate (Gb/s): 15.999299

- Max Peak to Peak Jitter: 28.449213 ps

- Total Jitter at BER of 10E-12: 34.595338 ps
  Total Jitter at BER of 10E-12 Passes Sigtest Limits!

- Minimum eye width: 27.904662 ps

- Deterministic Jitter Delta-Delta: 7.384714 ps
  Deterministic Jitter Delta-Delta Passes Sigtest Limits!

- Random Jitter (RMS): 1.934087 ps
  Random Jitter (RMS) Passes Sigtest Limits!

- Minimum Transition Eye Voltage: -0.134814 volts
  Minimum Transition Eye Voltage Passes Sigtest Limits!

- Maximum Transition Eye Voltage: 0.129074 volts
  Maximum Transition Eye Voltage Passes Sigtest Limits!

- Composite Eye Height: 0.071398

- Composite Eye Location: 0.508
  Composite Eye Height Passes Sigtest Limits!

- Extrapolated Eye Height: 0.052642
  Extrapolated Eye Height Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Above Eye: 0.033403 volts
  Minimum Transition Eye Voltage Margin Above Eye Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Below Eye: -0.045168 volts
  Minimum Transition Eye Voltage Margin Below Eye Passes Sigtest Limits!

- Minimum Transition Eye Height: 0.097571 volts

Worst Non Transition Signal Eye

TEMPLATE FILE SETTINGS

- Template File: PCIE_4_0_SYS \ PCIE_4_16GB_CEM_DUAL_PORT

- Nominal Data Rate (bits/sec): 15999999999.999998

- Target Unit Interval (s): 6.25e-011

- Minimum Time Allowed Between Crossovers (s): 4.0e-011

- Minimum Data For Testing (UI): 200

- Ambiguous UI Resolution Method: EYE_AMBIGUOUS_NONE (0)

- Tj@E-12 Peak to Peak Jitter Limit (s): 4.075e-011

- CTLE equalization index = 1

- DFE equalization: Tap 1 = 20.019531, Tap 2 = -8.300781

  Sigtest Version: 4.0.51