# Results for c:\Users\Administrator\Desktop\Project\G4PCIE_EX10_V2.00\PCIE Gen 4\PCIE 2\PCIE2_LANE 8_P0

Sigtest:

- Overall Sigtest Result: Pass!

- Mean Unit Interval (ps): 62.502842

- Min Time Between Crossovers (ps): 41.840685

- Data Rate (Gb/s): 15.999272

- Max Peak to Peak Jitter: 23.674293 ps

- Total Jitter at BER of 10E-12: 32.340305 ps
  Total Jitter at BER of 10E-12 Passes Sigtest Limits!

- Minimum eye width: 30.159695 ps

- Deterministic Jitter Delta-Delta: 5.890797 ps
  Deterministic Jitter Delta-Delta Passes Sigtest Limits!

- Random Jitter (RMS): 1.879988 ps
  Random Jitter (RMS) Passes Sigtest Limits!

- Minimum Transition Eye Voltage: -0.163929 volts
  Minimum Transition Eye Voltage Passes Sigtest Limits!

- Maximum Transition Eye Voltage: 0.153564 volts
  Maximum Transition Eye Voltage Passes Sigtest Limits!

- Composite Eye Height: 0.106206

- Composite Eye Location: 0.484
  Composite Eye Height Passes Sigtest Limits!

- Extrapolated Eye Height: 0.095949
  Extrapolated Eye Height Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Above Eye: 0.048606 volts
  Minimum Transition Eye Voltage Margin Above Eye Passes Sigtest Limits!

- Minimum Transition Eye Voltage Margin Below Eye: -0.059024 volts
  Minimum Transition Eye Voltage Margin Below Eye Passes Sigtest Limits!

- Minimum Transition Eye Height: 0.12663 volts

Worst Non Transition Signal Eye

TEMPLATE FILE SETTINGS

- Template File: PCIE_4_0_SYS \ PCIE_4_16GB_CEM_DUAL_PORT

- Nominal Data Rate (bits/sec): 15999999999.999998

- Target Unit Interval (s): 6.25e-011

- Minimum Time Allowed Between Crossovers (s): 4.0e-011

- Minimum Data For Testing (UI): 200

- Ambiguous UI Resolution Method: EYE_AMBIGUOUS_NONE (0)

- Tj@E-12 Peak to Peak Jitter Limit (s): 4.075e-011

- CTLE equalization index = 1

- DFE equalization: Tap 1 = 16.601562, Tap 2 = -13.183594

  Sigtest Version: 4.0.51