PCIE 3 LANE 4

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:36:37

# Test result summary

## Shows the test results as an overview

Product Number: | PCIe
Serial Number: |
Description: |
User Name: | Unknown User
User's Comment: |
Software Version: |
PCI Express N5990A ValiFrame | 3.5.4.1

Test name | Result
--- | ---
L0_Cal_16GTps_PS | Passed
L0_Cal_16GTps_DE | Passed
L0_Cal_16GTps_Vdiff | Passed
L0_Cal_16GTps_RJ | Passed
L0_Cal_16GTps_LFSJ | Passed
L0_Cal_16GTps_HFSJ | Passed
L0_Cal_16GTps_UI | Passed
L0_Cal_16GTps_IL | Passed
L0_Cal_16GTps_DMSI | Passed
L0_Cal_16GTps_CMSI | Passed
L0_Cal_16GTps_IniPres_EH | Passed
L0_Cal_16GTps_IniPres_EW | Passed
L0_Cal_16GTps_Chan_EH | Passed
L0_Cal_16GTps_Chan_EW | Passed
L0_Cal_16GTps_FinPres_EH | Passed
L0_Cal_16GTps_FinPres_EW | Passed
L0_Cal_16GTps_PreComp | Passed
L0_Cal_16GTps_CompEye | Passed
L0_Rx_16GTps_Comp | Passed

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:36:37

# Instrument Summary

## This table lists the instruments used to run these tests

Company | Instrument Name | Serial | Instrument Revision | Description
--- | --- | --- | --- | ---
Keysight Technologies | M8070B | MY57702122 | 8.0.280.26 | M8020 with integrated jitter sources for BER tests
Keysight Technologies | DSO Infiniium Series | Unknown | Unknown | Realtime scope for stress signal calibration

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:36:37

# L0_Cal_16GTps_PS

## for PCIe 4.0 System

----General---- |
Offline | False
EQ Calibration Pattern | EQ Two Pattern, 64 zeros, 64 ones
Verification Mode | False
Start With Minimum Loss Channel | False
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 32 GHz
Number of Waveform Averages | 256
Scope Connection for Calibration | Chan 1 3 Direct Connect
----​​​Generator---- |
Set Amplitude | 800 mV

Set Pre-Shoot [dB] | DE (-6 dB) [dB] | DE (-5 dB) [dB] | DE (-4 dB) [dB] | DE (-3 dB) [dB] | DE (-2 dB) [dB] | DE (-1 dB) [dB] | DE (0 dB) [dB]
--- | --- | --- | --- | --- | --- | --- | ---
0.00 | 0.39 | 0.37 | 0.32 | 0.29 | 0.26 | 0.24 | 0.22
1.00 | 1.37 | 1.33 | 1.27 | 1.34 | 1.27 | 1.22 | 1.19
2.00 | 2.44 | 2.42 | 2.41 | 2.36 | 2.30 | 2.29 | 2.24
3.00 | 3.45 | 3.42 | 3.44 | 3.44 | 3.39 | 3.29 | 3.25
4.00 | 4.56 | 4.48 | 4.49 | 4.45 | 4.41 | 4.40 | 4.31
5.00 | 5.62 | 5.67 | 5.49 | 5.48 | 5.49 | 5.42 | 5.34
6.00 | 6.62 | 6.61 | 6.62 | 6.58 | 6.59 | 6.49 | 6.45

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:36:37

# L0_Cal_16GTps_DE

## for PCIe 4.0 System

----General---- |
Offline | False
EQ Calibration Pattern | EQ Two Pattern, 64 zeros, 64 ones
Verification Mode | False
Start With Minimum Loss Channel | False
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 32 GHz
Number of Waveform Averages | 256
Scope Connection for Calibration | Chan 1 3 Direct Connect
----​​​Generator---- |
Set Amplitude | 800 mV

Set De-Emphasis [dB] | PS (0 dB) [dB] | PS (1 dB) [dB] | PS (2 dB) [dB] | PS (3 dB) [dB] | PS (4 dB) [dB] | PS (5 dB) [dB] | PS (6 dB) [dB]
--- | --- | --- | --- | --- | --- | --- | ---
-6.00 | -6.55 | -6.75 | -6.82 | -6.92 | -7.21 | -7.44 | -7.63
-5.00 | -5.54 | -5.64 | -5.89 | -6.06 | -6.26 | -6.62 | -6.83
-4.00 | -4.57 | -4.75 | -4.98 | -5.24 | -5.53 | -5.63 | -5.89
-3.00 | -3.56 | -3.80 | -4.10 | -4.40 | -4.54 | -4.78 | -5.09
-2.00 | -2.59 | -2.84 | -3.11 | -3.36 | -3.56 | -3.79 | -4.12
-1.00 | -1.58 | -1.94 | -2.16 | -2.46 | -2.72 | -2.96 | -3.22
0.00 | -0.50 | -0.87 | -1.18 | -1.39 | -1.67 | -1.94 | -2.24

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:36:37

# L0_Cal_16GTps_Vdiff

## for PCIe 4.0 System

----General---- |
Offline | False
EQ Calibration Pattern | EQ Two Pattern, 64 zeros, 64 ones
Verification Mode | False
Start With Minimum Loss Channel | False
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 32 GHz
Number of Waveform Averages | 256
Scope Connection for Calibration | Chan 1 3 Direct Connect
----​​​Generator---- |
Set Amplitude | 800 mV

Set Pre-Shoot [dB] | DE (-6 dB) [mV] | DE (-5 dB) [mV] | DE (-4 dB) [mV] | DE (-3 dB) [mV] | DE (-2 dB) [mV] | DE (-1 dB) [mV] | DE (0 dB) [mV]
--- | --- | --- | --- | --- | --- | --- | ---
0.00 | 929.00 | 923.00 | 930.00 | 924.00 | 925.00 | 926.00 | 925.00
1.00 | 919.00 | 920.00 | 922.00 | 926.00 | 926.00 | 922.00 | 923.00
2.00 | 923.00 | 923.00 | 922.00 | 921.00 | 921.00 | 924.00 | 929.00
3.00 | 919.00 | 923.00 | 925.00 | 924.00 | 920.00 | 921.00 | 922.00
4.00 | 920.00 | 923.00 | 921.00 | 923.00 | 926.00 | 926.00 | 926.00
5.00 | 918.00 | 924.00 | 926.00 | 922.00 | 922.00 | 926.00 | 922.00
6.00 | 922.00 | 925.00 | 919.00 | 921.00 | 924.00 | 922.00 | 925.00

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:39:00

# L0_Cal_16GTps_RJ

## for PCIe 4.0 System

----General---- |
Offline | False
Verification Mode | False
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 3
Number of UIs | 2 MUI
Scope Connection for Calibration | Chan 1 3 Direct Connect
----​​​Generator---- |
Pre-Shoot | 0 dB
De-Emphasis | 0 dB
Generator Voltage | 800 mV

Set Random Jitter [ps] | Measured Random Jitter [ps]
--- | ---
0.00 | 0.31
0.25 | 0.40
0.50 | 0.59
0.75 | 0.82
1.00 | 1.06
1.50 | 1.55
2.00 | 2.05
3.00 | 3.07
4.00 | 4.11

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:45:27

# L0_Cal_16GTps_LFSJ

## for PCIe 4.0 System

----General---- |
Offline | False
Verification Mode | False
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 3
Number of UIs | 2 MUI
Scope Connection for Calibration | Chan 1 3 Direct Connect
----​​​Generator---- |
Pre-Shoot | 0 dB
De-Emphasis | 0 dB
Generator Voltage | 800 mV

Set SJ [ps] | SJ (0.2 MHz) [ps] | SJ (0.5 MHz) [ps] | SJ (1 MHz) [ps] | SJ (2 MHz) [ps] | SJ (4 MHz) [ps]
--- | --- | --- | --- | --- | ---
6.25 | 6.25 | 6.20 | 6.12 | 6.08 | 6.09
12.50 | 12.50 | 11.96 | 11.93 | 11.96 | 12.01
25.00 | 23.92 | 24.31 | 24.36 | 24.29 | 24.26
50.00 | 47.82 | 49.70 | 49.40 | 49.32 | 49.21
100.00 | 96.39 | 99.32 | 98.95 | 99.07 | 99.13
200.00 | 193.27 | 198.74 | 199.23 | 198.57 | 198.96

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:49:13

# L0_Cal_16GTps_HFSJ

## for PCIe 4.0 System

----General---- |
Offline | False
Verification Mode | False
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 3
Number of UIs | 2 MUI
Scope Connection for Calibration | Chan 1 3 Direct Connect
----​​​Generator---- |
Pre-Shoot | 0 dB
De-Emphasis | 0 dB
Generator Voltage | 800 mV

Set SJ [ps] | SJ (5 MHz) [ps] | SJ (10 MHz) [ps] | SJ (100 MHz) [ps]
--- | --- | --- | ---
0.00 | 0.00 | 0.00 | 0.00
6.25 | 5.60 | 5.58 | 5.59
12.50 | 11.54 | 11.58 | 11.92
18.75 | 18.07 | 18.01 | 18.18
25.00 | 24.52 | 24.57 | 24.54

### Product Number: PCIe PCIe Station Unknown User 22/08/2022 10:50:06

# L0_Cal_16GTps_UI

## for PCIe 4.0 System

----General---- |
Offline | False
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 7
Number of UIs | 2 MUI
Scope Connection for Calibration | Chan 1 3 Direct Connect
----​​​Generator---- |
Pre-Shoot | 0 dB
De-Emphasis | 0 dB
Generator Voltage | 800 mV

Mean Unit Interval [ps]
62.500092973

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 18:06:12

# L0_Cal_16GTps_IL

## for PCIe 4.0 System

----General---- |
Offline | False
Measurement Method | VNA (manual)
Trace Loss Increment | -0.5 dB
Save Calibration Data | True
Start With Minimum Loss Channel | False
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 7
Number of Waveform Averages | 1024
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Variable ISI pairs---- |
CBB var. ISI pair | 11
CLB var. ISI pair -27dB Channel | 1
CLB var. ISI pair -28dB Channel | 1
CLB var. ISI pair -30dB Channel | 3

Frequency [GHz] | Insertion Loss (Trace 1) [dB] | Insertion Loss (Trace 2) [dB] | Insertion Loss (Trace 3) [dB]
--- | --- | --- | ---
1.00 | -4.70 | -4.95 | -5.20
1.10 | -5.03 | -5.29 | -5.55
1.20 | -5.37 | -5.64 | -5.91
1.30 | -5.70 | -5.98 | -6.26
1.40 | -6.03 | -6.32 | -6.62
1.50 | -6.36 | -6.67 | -6.97
1.60 | -6.70 | -7.01 | -7.33
1.70 | -7.03 | -7.36 | -7.68
1.80 | -7.36 | -7.70 | -8.03
1.90 | -7.70 | -8.04 | -8.39
2.00 | -8.03 | -8.39 | -8.74
2.10 | -8.36 | -8.73 | -9.10
2.20 | -8.69 | -9.07 | -9.45
2.30 | -9.03 | -9.42 | -9.81
2.40 | -9.36 | -9.76 | -10.16
2.50 | -9.69 | -10.10 | -10.51
2.60 | -10.03 | -10.45 | -10.87
2.70 | -10.36 | -10.79 | -11.22
2.80 | -10.69 | -11.13 | -11.58
2.90 | -11.02 | -11.48 | -11.93
3.00 | -11.36 | -11.82 | -12.29
3.10 | -11.69 | -12.17 | -12.64
3.20 | -12.02 | -12.51 | -12.99
3.30 | -12.36 | -12.85 | -13.35
3.40 | -12.69 | -13.20 | -13.70
3.50 | -13.02 | -13.54 | -14.06
3.60 | -13.35 | -13.88 | -14.41
3.70 | -13.69 | -14.23 | -14.77
3.80 | -14.02 | -14.57 | -15.12
3.90 | -14.35 | -14.91 | -15.47
4.00 | -14.69 | -15.26 | -15.83
4.10 | -15.02 | -15.60 | -16.18
4.20 | -15.35 | -15.94 | -16.54
4.30 | -15.68 | -16.29 | -16.89
4.40 | -16.02 | -16.63 | -17.25
4.50 | -16.35 | -16.98 | -17.60
4.60 | -16.68 | -17.32 | -17.95
4.70 | -17.02 | -17.66 | -18.31
4.80 | -17.35 | -18.01 | -18.66
4.90 | -17.68 | -18.35 | -19.02
5.00 | -18.01 | -18.69 | -19.37
5.10 | -18.35 | -19.04 | -19.73
5.20 | -18.68 | -19.38 | -20.08
5.30 | -19.01 | -19.72 | -20.43
5.40 | -19.35 | -20.07 | -20.79
5.50 | -19.68 | -20.41 | -21.14
5.60 | -20.01 | -20.75 | -21.50
5.70 | -20.34 | -21.10 | -21.85
5.80 | -20.68 | -21.44 | -22.21
5.90 | -21.01 | -21.79 | -22.56
6.00 | -21.34 | -22.13 | -22.91
6.10 | -21.68 | -22.47 | -23.27
6.20 | -22.01 | -22.82 | -23.62
6.30 | -22.34 | -23.16 | -23.98
6.40 | -22.67 | -23.50 | -24.33
6.50 | -23.01 | -23.85 | -24.69
6.60 | -23.34 | -24.19 | -25.04
6.70 | -23.67 | -24.53 | -25.39
6.80 | -24.01 | -24.88 | -25.75
6.90 | -24.34 | -25.22 | -26.10
7.00 | -24.67 | -25.56 | -26.46
7.10 | -25.00 | -25.91 | -26.81
7.20 | -25.34 | -26.25 | -27.17
7.30 | -25.67 | -26.60 | -27.52
7.40 | -26.00 | -26.94 | -27.87
7.50 | -26.34 | -27.28 | -28.23
7.60 | -26.67 | -27.63 | -28.58
7.70 | -27.00 | -27.97 | -28.94
7.80 | -27.33 | -28.31 | -29.29
7.90 | -27.67 | -28.66 | -29.65
8.00 | -28.00 | -29.00 | -30.00

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 18:11:49

# L0_Cal_16GTps_DMSI

## for PCIe 4.0 System

----General---- |
Offline | False
Verification Mode | False
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Waveform Averages | 128
Horizontal Range | 40 ns
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CLB var. ISI pair | 1
CBB var. ISI pair | 11
Total Channel Loss | -28 dB

Set DMSI [mV] | Measured DMSI [mV]
--- | ---
0.00 | 0.17
5.00 | 4.06
10.00 | 9.65
15.00 | 14.56
20.00 | 19.46
30.00 | 29.28
40.00 | 39.10
50.00 | 48.93

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 18:20:05

# L0_Cal_16GTps_CMSI

## for PCIe 4.0 System

----General---- |
Offline | False
Verification Mode | False
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Waveform Averages | 128
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CLB var. ISI pair | 1
Total Channel Loss | -28 dB

Set CMSI [mV] | Measured CMSI [mV]
--- | ---
0.00 | 0.11
100.00 | 47.93
200.00 | 96.49
300.00 | 144.05
400.00 | 191.50
500.00 | 241.79
600.00 | 293.39

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 20:09:15

# L0_Cal_16GTps_IniPres_EH

## for PCIe 4.0 System

----General---- |
Offline | False
Equalization Preset Range | P5;P6
CTLE Start Value | -9.75 dB
CTLE Stop Value | -8.75 dB
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 7
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CLB var. ISI pair | 3
CBB var. ISI pair | 11
Total Channel Loss | -30 dB
----​​​Generator---- |
Generator Launch Voltage | 800 mV
DMSI | 14 mV
Random Jitter | 1 ps
Sinusoidal Jitter | 6.25 ps
Sinusoidal Jitter Frequency | 100 MHz

Set Equalization Preset [] | Measured Eye Height (-9.75 dB CTLE) [mV] | Measured Eye Height (-9.5 dB CTLE) [mV] | Measured Eye Height (-9.25 dB CTLE) [mV] | Measured Eye Height (-9 dB CTLE) [mV] | Measured Eye Height (-8.75 dB CTLE) [mV]
--- | --- | --- | --- | --- | ---
5.00 | 12.81 | 16.10 | 16.30 | 17.20 | 18.43
6.00 | 14.22 | 13.13 | 19.00 | 19.04 | 18.65

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 20:09:15

# L0_Cal_16GTps_IniPres_EW

## for PCIe 4.0 System

----General---- |
Offline | False
Equalization Preset Range | P5;P6
CTLE Start Value | -9.75 dB
CTLE Stop Value | -8.75 dB
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 7
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CLB var. ISI pair | 3
CBB var. ISI pair | 11
Total Channel Loss | -30 dB
----​​​Generator---- |
Generator Launch Voltage | 800 mV
DMSI | 14 mV
Random Jitter | 1 ps
Sinusoidal Jitter | 6.25 ps
Sinusoidal Jitter Frequency | 100 MHz

Set Equalization Preset [] | Measured Eye Width (-9.75 dB CTLE) [ps] | Measured Eye Width (-9.5 dB CTLE) [ps] | Measured Eye Width (-9.25 dB CTLE) [ps] | Measured Eye Width (-9 dB CTLE) [ps] | Measured Eye Width (-8.75 dB CTLE) [ps]
--- | --- | --- | --- | --- | ---
5.00 | 18.74 | 20.32 | 21.00 | 22.63 | 23.63
6.00 | 18.66 | 19.50 | 21.57 | 21.85 | 23.27

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 20:23:25

# L0_Cal_16GTps_Chan_EH

## for PCIe 4.0 System

----General---- |
Offline | False
Trace Number Start Value | 3
Trace Number Stop Value | 0
CTLE Start Value | -9.75 dB
CTLE Stop Value | -8.75 dB
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 7
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CBB var. ISI pair | 11
----​​​Generator---- |
Pre-Shoot | 1.9 dB
De-Emphasis | 0 dB
Generator Launch Voltage | 800 mV
DMSI | 14 mV
Random Jitter | 1 ps
Sinusoidal Jitter | 6.25 ps
Sinusoidal Jitter Frequency | 100 MHz

Set CLB var. ISI pair [] | Measured Eye Height (-9.75 dB CTLE) [mV] | Measured Eye Height (-9.5 dB CTLE) [mV] | Measured Eye Height (-9.25 dB CTLE) [mV] | Measured Eye Height (-9 dB CTLE) [mV] | Measured Eye Height (-8.75 dB CTLE) [mV]
--- | --- | --- | --- | --- | ---
3.00 | 12.81 | 16.10 | 16.30 | 17.20 | 18.43

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 20:23:25

# L0_Cal_16GTps_Chan_EW

## for PCIe 4.0 System

----General---- |
Offline | False
Trace Number Start Value | 3
Trace Number Stop Value | 0
CTLE Start Value | -9.75 dB
CTLE Stop Value | -8.75 dB
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 7
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CBB var. ISI pair | 11
----​​​Generator---- |
Pre-Shoot | 1.9 dB
De-Emphasis | 0 dB
Generator Launch Voltage | 800 mV
DMSI | 14 mV
Random Jitter | 1 ps
Sinusoidal Jitter | 6.25 ps
Sinusoidal Jitter Frequency | 100 MHz

Set CLB var. ISI pair [] | Measured Eye Width (-9.75 dB CTLE) [ps] | Measured Eye Width (-9.5 dB CTLE) [ps] | Measured Eye Width (-9.25 dB CTLE) [ps] | Measured Eye Width (-9 dB CTLE) [ps] | Measured Eye Width (-8.75 dB CTLE) [ps]
--- | --- | --- | --- | --- | ---
3.00 | 18.74 | 20.32 | 21.00 | 22.63 | 23.63

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 21:49:08

# L0_Cal_16GTps_FinPres_EH

## for PCIe 4.0 System

----General---- |
Offline | False
Equalization Preset Range | P5;P6
CTLE Start Value | -9.75 dB
CTLE Stop Value | -8.75 dB
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 7
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CLB var. ISI pair | 3
CBB var. ISI pair | 11
Total Channel Loss | -30 dB
----​​​Generator---- |
Generator Launch Voltage | 800 mV
DMSI | 14 mV
Random Jitter | 1 ps
Sinusoidal Jitter | 6.25 ps
Sinusoidal Jitter Frequency | 100 MHz

Set Equalization Preset [] | Measured Eye Height (-9.75 dB CTLE) [mV] | Measured Eye Height (-9.5 dB CTLE) [mV] | Measured Eye Height (-9.25 dB CTLE) [mV] | Measured Eye Height (-9 dB CTLE) [mV] | Measured Eye Height (-8.75 dB CTLE) [mV]
--- | --- | --- | --- | --- | ---
5.00 | 13.26 | 15.02 | 17.71 | 18.89 | 19.70
6.00 | 13.91 | 13.31 | 19.28 | 16.42 | 20.43

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 21:49:08

# L0_Cal_16GTps_FinPres_EW

## for PCIe 4.0 System

----General---- |
Offline | False
Equalization Preset Range | P5;P6
CTLE Start Value | -9.75 dB
CTLE Stop Value | -8.75 dB
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 7
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CLB var. ISI pair | 3
CBB var. ISI pair | 11
Total Channel Loss | -30 dB
----​​​Generator---- |
Generator Launch Voltage | 800 mV
DMSI | 14 mV
Random Jitter | 1 ps
Sinusoidal Jitter | 6.25 ps
Sinusoidal Jitter Frequency | 100 MHz

Set Equalization Preset [] | Measured Eye Width (-9.75 dB CTLE) [ps] | Measured Eye Width (-9.5 dB CTLE) [ps] | Measured Eye Width (-9.25 dB CTLE) [ps] | Measured Eye Width (-9 dB CTLE) [ps] | Measured Eye Width (-8.75 dB CTLE) [ps]
--- | --- | --- | --- | --- | ---
5.00 | 18.90 | 20.00 | 21.41 | 22.90 | 23.04
6.00 | 18.57 | 20.54 | 21.00 | 22.60 | 22.87

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 23:12:18

# L0_Cal_16GTps_PreComp

## for PCIe 4.0 System

----General---- |
Offline | False
CTLE | -8.75 dB
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 21
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CLB var. ISI pair | 3
CBB var. ISI pair | 11
Total Channel Loss | -30 dB
----​​​Generator---- |
Pre-Shoot | 2.5 dB
De-Emphasis | 0 dB
Random Jitter | 1 ps

DMSI [mV] | SJ [ps] | Vdiff [mV] | Eye Height [mV] | Eye Width [ps]
--- | --- | --- | --- | ---
14.0 | 6.25 | 800 | 20.81 | 23.40
25.0 | 6.25 | 800 | 13.19 | 18.76
14.0 | 10.00 | 800 | 14.59 | 19.32
14.0 | 6.25 | 720 | 15.78 | 21.26

### Product Number: PCIe PCIe Station Unknown User 29/08/2022 23:34:12

# L0_Cal_16GTps_CompEye

## for PCIe 4.0 System

----General---- |
Offline | False
CTLE | -8.75 dB
Start With Minimum Loss Channel | False
SigTest Version | 4.0.52
Oscilloscope | Keysight DSO, DSAV334A, SN: MY57500102, FW rev.: 06.60.00601, Used for Calibration
BERT System | Keysight M8020A J-BERT, M8070B, SN: MY57702122
Generator Channel Channel | M1.DataOut1
----​​Oscilloscope---- |
Scope Bandwidth | 25 GHz
Number of Averages | 21
Number of UIs | 2 MUI
Gen4 Transfer Function File for Package Model on Scope | PCIe4RxPackageModel_RootComplex_v2.tf4
Scope Connection for Calibration | Chan 1 3 Direct Connect
----Channel---- |
CLB var. ISI pair | 3
CBB var. ISI pair | 11
Total Channel Loss | -30 dB
----​​​Generator---- |
Pre-Shoot | 2.5 dB
De-Emphasis | 0 dB
Sinusoidal Jitter Frequency | 100 MHz
Random Jitter | 1 ps
----Search Algorithm---- |
Minimum Vdiff | 720 mV
Maximum DMSI | 25 mV
Maximum SJ | 10 ps
Max Number of Search Steps | 7
Use nominal EH/EW results from Pre Comp Cal | True

DMSI [mV] | SJ [ps] | Vdiff [mV] | Eye Height [mV] | Eye Width [ps]
--- | --- | --- | --- | ---
15.2 | 9.85 | 800 | 14.67 | 18.84

### Product Number: PCIe PCIe Station Unknown User 20/10/2022 14:24:08

# L0_Rx_16GTps_Comp

## for PCIe 4.0 System

----General---- |
Offline | False
BER Mode | FixedTime
BER Measurement Duration | 62.5 s
Allowed Bit Error | 1
Pause before Auto-Align | False
----Channel---- |
CLB var. ISI pair | 3
Total Channel Loss | -30 dB
----​​​Impairments---- |
Residual SSC | 0 s
Random Jitter | 1 ps
Sinusoidal Jitter | 9.85 ps
Sinusoidal Jitter Frequency | 100 MHz
Common Mode Sinusoidal Interference | 150 mV
Differential Mode Sinusoidal Interference | 15.2 mV
Generator Launch Voltage | 800 mV
----Link Training---- |
Enable Impairments for Loopback Training | True
----​Equalization---- |
Use Preset | True
Generator Preset | P5
Pre-Shoot | 1.9 dB
De-Emphasis | 0 dB
----​​​​​​​​​​​​​​​​​Loopback Training---- |
Link Training Mode | Vendor Specific
Link Training Suite Settings File | C:\ProgramData\BitifEye\ValiFrameK0\PCIe\Settings\TrainingScripts\Pcie4_16G_M8020A_Loopback_VendorSpecific.txt
Suppress Loopback Training Messages | False
----​​​​​​​​​​​​​​​​Interactive Link Training---- |
Training through | L0-Recovery
Generator Full Swing | 24
DUT Target Preset | P7
DUT Target Preset Gen4 | P7
Speed Change Control | BERT
Drop Link Method | LTSSM
----​​​​​​​​​​​​​​​Error Detector---- |
Use CDR | True
CDR Loop Bandwidth | 20 MHz
Peaking | 1 dB
Analyzer Equalization | -9 dB
Sensitivity | High
Polarity | Normal
----​​​​BER Measurement---- |
Relax Time | 3 s

Result | Sinusoidal Jitter Frequency [MHz] | Sinusoidal Jitter [ps] | Allowed Bit Errors [] | Measured Bit Errors []
--- | --- | --- | --- | ---
pass | 100.0 | 9.85 | 1 | 0