{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Overview","Thermal & EDP","NVQual Test Results","System Images"],"not_rendered":{"charts":0,"images":10,"macros":1,"external_links":0,"defined_names":69,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Overview","index":0,"n_rows":20,"n_cols":16,"rows_kept":20,"cut":false,"hidden":false,"merged":[[3,2,3,11]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Template Version ",null,"v01"]
[null,null,"NVQual Report "]
[]
[null,"Instructions:","This template is intended to be used by OEM/ODM/system integrators for NVIDIA product qualification."]
[null,null,"This report should be populated in full and then submitted to NVIDIA for review and approval."]
[null,null,"ALL DATA REQUIRED FROM THE CUSTOMER IS HIGHLIGHTED IN YELLOW CELLS"]
[null,"Product SKU ","PG500 SKU 200 & SKU 202"]
[null,"Product Brand","Tesla V100 PCIe"]
[null,"Date:","2018-06-26"]
[]
[null,"Project Information "]
[]
[null,"Project Name","3U10G-F/C621"]
[null,"Partner","ASRock Rack"]
[null,"ODM"]
[null,"System Model Name"]
[]
[]
[null,"Specifications in this worksheet are subject to change.  Please check with NVIDIA to ensure you are using the latest values."]
[null,"This entire Excel Workbook is \"NVIDIA Confidential.\""]

{"sheet":"Thermal & EDP","index":1,"n_rows":39,"n_cols":12,"rows_kept":39,"cut":false,"hidden":false,"merged":[[35,5,35,6],[36,5,36,6],[37,5,37,6],[29,2,38,2],[29,3,29,4],[30,3,30,4],[31,3,31,4],[32,3,32,4],[33,3,33,4],[34,3,34,4],[35,3,35,4],[36,3,36,4],[37,3,37,4],[38,3,38,4],[38,5,38,6],[31,5,31,6],[1,1,1,2],[12,3,12,4],[9,2,10,2],[25,8,25,9],[26,8,26,9],[12,9,12,10],[12,5,12,6],[18,7,19,14],[25,2,28,2],[25,3,25,4],[26,3,26,4],[27,3,27,4],[28,3,28,4],[27,8,27,9],[25,5,25,6],[13,2,16,2],[32,5,32,6],[33,5,33,6],[34,5,34,6],[26,5,26,6],[27,5,27,6],[28,5,28,6],[29,5,29,6],[30,5,30,6],[29,8,29,9],[28,8,28,9],[35,8,35,9],[36,8,36,9],[37,8,37,9],[38,8,38,9],[30,8,30,9],[31,8,31,9],[32,8,32,9],[33,8,33,9],[34,8,34,9]]}
["Qualification"]
[]
[null,"Power Qualification"]
[]
[null,null,"Instructions"]
[null,null,"- Record the following data with all graphics boards populated in a single chassis (rack/blade) using an oscilloscope. The system loading should match the production configuration. "]
[null,null,"- Recommended to run the NVQual InputEDPp test at ambient room temperature"]
[null,null,"- Only the worst case GPU Temperature (Tj) and Input Power reported should be captured in the table below. "]
[]
[null,null,"Test Condition ","Background NVQual Test","Temperature "]
[null,null,null,8,"35 deg C"]
[]
[null,null,null,"Input Voltage",null,"Tolerance",null,null,null,"Measured Voltage",null,"Comments"]
[null,null,"NVQual InputEDPp\n","Voltage Rail","Description","Min","Max","Min","Max","Min","Max"]
[null,null,null,"PEX 3V3","PCIe Edge",-0.09,0.09,{"$f":"3.3+(3.3*F15)","v":3.0029999999999997},{"$f":"3.3+(3.3*G15)","v":3.597},"3.33 V","3.55 V"]
[null,null,null,"PEX 12V","PCIe Edge",-0.08,0.08,{"$f":"12+(12*F16)","v":11.04},12.96,"11.7 V","12.7 V"]
[null,null,null,"CPU 8PIN","CPU 8PIN",-0.08,0.08,{"$f":"12+(12*F17)","v":11.04},{"$f":"12+(12*G17)","v":12.96},"11.7 V","12.7 V"]
[]
[]
[]
[null,"Thermal Qualification"]
[]
[null,null,"Instructions"]
[null,null,"- Record details related to your system setup for NVQual Thermal Qualification Test (MTT) - Test #1 "]
[]
[null,null,"Environment for Cooling","Item",null,"Description",null,"Customer Results","Comments"]
[null,null,null,"Card cooler type",null,"Passive, Active or Water Cooled",null,"Passive"]
[null,null,null,"Card orientation wrt airflow",null,"Left-to-right, Right-to-left, etc.",null,"Left-to-right"]
[null,null,null,"Airflow bypass at this card",null,"% bypass",null,"about 10%"]
[null,null,"Air Measurements"," Chassis inlet ambient temperature ",null,"Customer’s max specified ambient temperature (outside system chassis)",null,"35C"]
[null,null,null,"System external ambient temperature as measured during MTT test",null,"External ambient temperature measurement during test run",null,"35.1C"]
[null,null,null,"heatsink inlet air temperature (maximum) during NVQual MTT execution",null,"maximum inlet temperature during the MTT",null,"35.3\n35.1\n34.9","Please describe how measured. 3 thermocouples? List individual temperatures from each sensor used."]
[null,null,null,"Airflow measurement point",null,"Select: Card inlet, card outlet, entire chassis",null,"Entire Chassis"]
[null,null,null,"Flow rate measured or estimated?",null,"Select measured or estimated.",null,"Estimated"]
[null,null,null,"If measured, how?",null,"Single card measurement or full chassis",null,"N/A","Please provide details of how measurement was performed"]
[null,null,null,"If estimated, how?",null,"From previous GPU card? Previous chassis?",null,"From previous GPU card(M40)","Please provide details of how estimate was performed"]
[null,null,null,"Air flow rate in CFM",null,"CFM through cooler in decimal",null,150]
[null,null,null,"System Fans PWM% during test run",null,"System fans PWM% during test (during steady state portion of test)",null,1]
[null,null,null,"System Fans max allowable PWM%",null,"Maximum shippable PWM% of system fans",null,1]

{"sheet":"NVQual Test Results","index":2,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"NVQual Test Results "]
[]
[null,"Instructions"]
[null,"- The Qualification requirements list the minimum requirements. System refers to a fully populated production-level system"]
[null,"- Customer Result should include Pass, Fail or Did not complete. Comments can be used to provide more details."]
[null,"- NVQual creates a folder for each test. Once you meet the qualification requirements, please zip individual test folders and attach them to this spreadsheet. \n"]
[null,"- If the qualification requires logs from 5 systems (minimum), then make sure the zip archived test folder contains all the logs for each system. \n"]
[null,"- NVIDIA recommends that all (min.) five systems use different boards. If the required number of boards is not available, then it is acceptable to move modules between systems being tested."]
[null,"- All samples should be QS or later unless otherwise specified. "]
[]
[null,"NVQual Test Item","NVQual Test Name","Qualification Requirements ","Customer Results","Comments\nPlease add details regarding \nspecific issues here."]
[null,"Test #1 ","Thermal Qualification Test (MTT)","Minimum Systems: 1 or more\nTest Condition: Refer to airflow requirements\nMinimum Loops: 1 or more"]
[null,"Test #2","PCI Express Qualification Test","Minimum Systems: 5 or more\nTest Condition: Room temperature\nMinimum Loops: 1 or more"]
[null,"Test #3","PCI Express Bandwidth Test","Minimum Systems: 1 or more\nTest Condition: Room temperature\nMinimum Loops: 1 or more"]
[null,"Test #7","Input EDPp Test","Minimum Systems: 5 or more\nTest Condition: Room temperature\nMinimum Loops: 1 or more"]
[null,"Test #11","PCI Express Data Eye Metric","Minimum Systems: 5 or more\nTest Condition: Room temperature\nMinimum Loops: 1 or more"]

{"sheet":"System Images","index":3,"n_rows":192,"n_cols":3,"rows_kept":192,"cut":false,"hidden":false,"merged":[[1,1,1,2]]}
["System Images "]
[]
[null,"Import System Images"]
[]
[null,"Instructions"]
[null,"Please attach photos of the following:"]
[null,"- All board locations in chassis, indicating each board location and chassis air inlet location."]
[null,"- For thermal qualification, indicate airflow inlet to the worst-case board location, heat sink inlet temperature measurement location, and airflow measurement location"]
[null,"- Chassis placement in cabinet or rack (if applicable), indicating worst-case chassis location for thermal qualification, and airflow direction."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Import Scopeshots"]
[]
[null,"Instructions"]
[null,"Please attach photos of the following:"]
[null,"- Scopeshot running InputEDPp Test #7 for worst case transisents at room temperature measuring 12V input voltage and current. "]
[null,"- Current measurements can be waived if there is no way to put current loops in the system."]
[null,"- Turn on measure statistics and keep capturing through the entire Input EDPp test on a single scope shot."]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Import System Topology"]
[]
[null,"Instructions"]
[null,"Please attach system topology generated in NVQual"]
[null,"- All board locations in chassis, run system topology tool in NVQual."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Attachment History"]
[null,"Type","Filename"]
[null,"system","C:\\Users\\hgill\\Pictures\\rzoKRY5lVgxa8hX3_setting_fff_1_90_end_500.jpg"]
[null,"scopeshot","C:\\Users\\hgill\\Pictures\\11177_big.png"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"hello"]