

**PLX SOP**


**How to check the speed of PCIE Upstream and Downstream**


Prepare:

1. JavaSetup8u40.exe
2. PLX\_SDK\_v7\_11\_Final\_2014-03-04.exe
3. AsRock\_8747-8748-8732.lic

Steps:


1. Install JAVA
2. Install “PLX\_SDK\_v7\_11\_Final\_2014-03-04.exe”
3. Execute “PLX Device Editor”
4. Select License file and load it.





1. Execute “PLX Device Editor”.

Check value of port 0(upstream) port 8(downstream) and port 16(downstream)



依序點選左邊四個欄位

確認Port0/8/16的值各為多少

